# Ceph Setup Issue - Configuration Mismatch

**Date**: 2025-12-15  
**Issue**: Cannot add r630-01 monitor due to configuration mismatch

## Problem

When attempting to add r630-01 as a Ceph monitor, we discovered:

1. **Different FSIDs**: 
   - ML110-01 cluster: `f601f0e2-cd09-402f-9e15-4b1c9a7a7b25` (from earlier status)
   - R630-01 config: `021d20d3-446f-42cb-a219-5e01213b7b2d` (from current /etc/pve/ceph.conf)

2. **Network Configuration Mismatch**:
   - ML110-01: `192.168.11.0/24`
   - R630-01: `192.168.11.11/24` (incorrect - should be 192.168.11.0/24)

3. **Monitor Connection Issues**:
   - ML110-01 monitor is running but commands timeout
   - Cannot get monmap from ml110-01
   - R630-01 cannot connect to cluster

## Root Cause

The `/etc/pve/ceph.conf` on r630-01 appears to have a different/incorrect configuration, possibly from a previous cluster setup or misconfiguration. The Proxmox cluster filesystem should sync this, but there may be a conflict.

## Solution Options

### Option 1: Sync Configuration from ML110-01
Since Proxmox cluster filesystem should sync `/etc/pve/ceph.conf`, we need to ensure:
1. ML110-01 has the correct configuration
2. Configuration syncs to r630-01
3. Then add r630-01 monitor

### Option 2: Reinitialize Ceph Cluster
If the cluster on ml110-01 is not operational or has issues:
1. Stop Ceph on ml110-01
2. Reinitialize with proper configuration
3. Add r630-01 monitor
4. Add OSDs

### Option 3: Use Proxmox Web UI
The Proxmox web interface may handle the configuration and monitor addition more reliably.

## Current Status

- ML110-01: Monitor running but cluster commands timeout
- R630-01: Cannot connect to cluster, configuration mismatch
- Need to resolve configuration before proceeding

