# Ceph Cluster Status - sfvalley-01

**Date**: 2025-12-15  
**Last Updated**: 2025-12-15

## Summary

✅ **Ceph Installation**: Complete on both servers  
⚠️ **Cluster Configuration**: Monitor on r630-01 needs to be added to existing cluster  
📝 **Cluster Name**: sfvalley-01 (to be configured)

## Installation Status

### ML110-01 (192.168.11.10)
- ✅ Ceph packages installed (19.2.3-pve2)
- ✅ Monitor service: **ACTIVE** (ml110-01)
- ✅ Manager service: **ACTIVE** (ml110-01)
- ✅ Cluster FSID: f601f0e2-cd09-402f-9e15-4b1c9a7a7b25

### R630-01 (192.168.11.11)
- ✅ Ceph packages installed (19.2.3-pve2)
- ❌ Monitor service: **FAILED** (needs filesystem creation)
- ⚠️ Manager service: Not yet configured
- ⚠️ Needs to join existing cluster

## Next Steps

1. **Add r630-01 monitor to cluster** (see CEPH_CLUSTER_SETUP.md for commands)
2. **Verify quorum** once both monitors are running
3. **Configure cluster name** as "sfvalley-01" if required
4. **Add OSDs** using available disks (6x 250GB SSDs on r630-01)

## Commands Reference

```bash
# Check cluster status
ceph -s

# Check monitor status
systemctl status ceph-mon@ml110-01.service
systemctl status ceph-mon@r630-01.service

# Check monitor quorum
ceph quorum_status

# List monitors
ceph mon dump
```

