# Complete Status Report - sfvalley-01 Cluster

**Date**: 2025-12-15 14:55 PST  
**Cluster Name**: sfvalley-01  
**Report Type**: Pre-Change Status Poll

## Proxmox Cluster Status

### ✅ **HEALTHY - Quorum Established**

**Cluster Information:**
- **Name**: sfvalley-01
- **Config Version**: 2
- **Transport**: knet
- **Secure Auth**: Enabled

**Quorum Status:**
- **Status**: ✅ Quorate
- **Expected Votes**: 2
- **Total Votes**: 2
- **Quorum**: 2

**Cluster Members:**
- **Node 1**: ml110-01 (192.168.11.10) - Node ID: 0x00000001
- **Node 2**: r630-01 (192.168.11.11) - Node ID: 0x00000002

**Status**: ✅ Both nodes are active and in quorum

---

## Ceph Cluster Status

### ⚠️ **PARTIALLY OPERATIONAL - Monitor Issues**

**Cluster Configuration:**
- **FSID**: f601f0e2-cd09-402f-9e15-4b1c9a7a7b25
- **Network**: 192.168.11.0/24 (public and cluster)
- **Pool Settings**: 
  - Default size: 3
  - Default min_size: 2

### ML110-01 (192.168.11.10) Status

**Services:**
- ✅ **ceph-mon@ml110-01.service**: ACTIVE (running)
  - Status: Running but in "probing" state
  - Started: Mon 2025-12-15 14:39:30 PST
  - Memory: 142.7M
  - Issue: Reporting slow operations (1800+ slow ops)
  
- ✅ **ceph-mgr@ml110-01.service**: ACTIVE (running)
  - Status: Running
  - Started: Mon 2025-12-15 14:39:33 PST
  - Memory: 327.3M
  - Issue: Authentication errors with monitor

**Data Directories:**
- ✅ `/var/lib/ceph/mon/ceph-ml110-01/` - Exists
- ✅ `/var/lib/ceph/mgr/ceph-ml110-01/` - Exists
- ⚠️ `/var/lib/ceph/osd/` - Empty (no OSDs)

### R630-01 (192.168.11.11) Status

**Services:**
- ❌ **ceph-mon@r630-01.service**: FAILED
  - Status: Failed (exit-code)
  - Error: Monitor data directory does not exist - needs 'mkfs'
  - Last attempt: Mon 2025-12-15 14:43:39 PST
  - Issue: Monitor filesystem not created
  
- ✅ **ceph-mgr@r630-01.service**: ACTIVE (running)
  - Status: Running
  - Started: Mon 2025-12-15 14:39:47 PST
  - Memory: 326M
  - Issue: Reporting status from non-daemon mon.r630-01

**Data Directories:**
- ⚠️ `/var/lib/ceph/mon/ceph-r630-01/` - Exists but EMPTY (needs mkfs)
- ✅ `/var/lib/ceph/mgr/ceph-r630-01/` - Exists
- ⚠️ `/var/lib/ceph/osd/` - Empty (no OSDs)

### Ceph Cluster Access

**Status**: ⚠️ **TIMEOUT ISSUES**
- `ceph -s`: Timeout
- `ceph mon dump`: Timeout
- `ceph osd tree`: Timeout
- `pveceph status`: Timeout

**Root Cause**: Monitor on ml110-01 is in "probing" state and cannot form quorum without r630-01 monitor. This causes all Ceph commands to timeout.

---

## Configuration Files

### `/etc/pve/ceph.conf` (Synced across cluster)

Both nodes have identical configuration:
```
[global]
	auth_client_required = cephx
	auth_cluster_required = cephx
	auth_service_required = cephx
	cluster_network = 192.168.11.0/24
	fsid = f601f0e2-cd09-402f-9e15-4b1c9a7a7b25
	mon_allow_pool_delete = true
	mon_host = 192.168.11.10
	ms_bind_ipv4 = true
	ms_bind_ipv6 = false
	osd_pool_default_min_size = 2
	osd_pool_default_size = 3
	public_network = 192.168.11.0/24

[client]
	keyring = /etc/pve/priv/$cluster.$name.keyring

[client.crash]
	keyring = /etc/pve/ceph/$cluster.$name.keyring

[mon.ml110-01]
	public_addr = 192.168.11.10
```

**Note**: Configuration only lists ml110-01 in mon_host. r630-01 monitor needs to be added.

---

## Issues Identified

### Critical Issues

1. **R630-01 Monitor Not Operational**
   - Monitor service failed
   - Monitor filesystem not created
   - Needs: `ceph-mon --mkfs` to create filesystem
   - Impact: No quorum, cluster commands timeout

2. **Monitor Quorum Not Established**
   - Only 1 monitor running (ml110-01)
   - ml110-01 monitor in "probing" state
   - Cannot form quorum with single monitor
   - Impact: Cluster inaccessible

3. **Ceph Commands Timing Out**
   - All `ceph` commands timeout
   - Cannot query cluster status
   - Impact: Cannot manage cluster

### Warning Issues

1. **No OSDs Configured**
   - No OSDs on either node
   - Cluster has no storage
   - Impact: Cannot store data

2. **Monitor Configuration Incomplete**
   - `mon_host` only lists ml110-01
   - r630-01 monitor not in configuration
   - Impact: r630-01 monitor cannot be discovered

3. **Slow Operations on Monitor**
   - ml110-01 monitor reporting 1800+ slow operations
   - May indicate performance issues
   - Impact: Degraded performance

---

## Required Actions

### Priority 1: Fix R630-01 Monitor (CRITICAL)

**Steps:**
1. Get monmap and keyring from ml110-01
2. Create monitor filesystem on r630-01
3. Start monitor service
4. Verify quorum established

**Commands:**
```bash
# On ml110-01
ceph mon getmap -o /tmp/monmap
scp /tmp/monmap root@192.168.11.11:/tmp/
scp /etc/pve/priv/ceph.mon.keyring root@192.168.11.11:/tmp/mon-keyring

# On r630-01
mkdir -p /var/lib/ceph/mon/ceph-r630-01
chown ceph:ceph /var/lib/ceph/mon/ceph-r630-01
ceph-mon --mkfs -i r630-01 --monmap /tmp/monmap --keyring /tmp/mon-keyring
chown -R ceph:ceph /var/lib/ceph/mon/ceph-r630-01
systemctl start ceph-mon@r630-01.service
```

### Priority 2: Update Monitor Configuration

**Steps:**
1. Add r630-01 to mon_host in ceph.conf
2. Add [mon.r630-01] section
3. Verify configuration syncs to both nodes

### Priority 3: Verify Quorum

**Steps:**
1. Check monitor quorum: `ceph quorum_status`
2. Verify both monitors in quorum
3. Test cluster access: `ceph -s`

### Priority 4: Add OSDs

**Steps:**
1. Identify available disks (6x 250GB SSDs on r630-01)
2. Create OSDs using `pveceph osd create`
3. Verify OSD status

---

## Summary

### ✅ Working
- Proxmox cluster: Healthy, quorum established
- Ceph packages: Installed on both nodes
- Ceph manager: Running on both nodes
- Ceph monitor: Running on ml110-01
- Configuration: Synced across cluster

### ⚠️ Needs Attention
- Ceph monitor: r630-01 monitor needs filesystem creation
- Monitor quorum: Cannot form quorum with single monitor
- Cluster access: Commands timing out
- OSDs: No OSDs configured

### ❌ Blocking Issues
- R630-01 monitor not operational (blocks quorum)
- Cluster commands timing out (blocks management)

---

## Next Steps

1. **Fix r630-01 monitor** (see Priority 1 above)
2. **Update monitor configuration** to include r630-01
3. **Verify quorum** and cluster access
4. **Add OSDs** once cluster is operational
5. **Monitor performance** for slow operations

---

## Notes

- Proxmox cluster "sfvalley-01" is healthy and operational
- Ceph cluster exists but needs monitor quorum to be fully operational
- All configuration is synced via Proxmox cluster filesystem
- Both nodes have Ceph installed and partially configured
- Once monitor quorum is established, cluster should become fully accessible

